**INSTALLATION INSTRUCTIONS**

**Applicable Models**

CHB190 Chevy "NEW" Silverado LT1500 2007 - UP

CHR190 Chevy "NEW" Silverado LT1500 2007 - UP W/Rake

**Steps**

Remove original bumper (Remove outer bumper brackets and 2 through frame bolts)

Remove tow hook bolts from outside of frame (2 on passenger side, 1 on driver side)

Install Ali Arc bumper to outside of frame and fasten using original bolts.

There will be 4 bolts on the passenger side and 3 bolts on the driver side

Align the Ali Arc bumper before securely tightening bolts.

**Cleaning and Maintenance**

Use soap and water. Avoid acid washes, as it will etch aluminum surfaces.

Original shine can be maintained by periodically using a standard metal polish.

We use and recommend Autosol.